A Real-Time (or) Field-based Research Project Report

on

**ULTRASONIC SPECTACLES AND WAIST BELT FOR VISUALLY IMPAIRED AND BLIND PERSON**

submitted in partial fulfillment of the requirements for the award of the degree of

**Bachelor of Technology**

in

**COMPUTER SCIENCE AND ENGINEERING**

by B.BHARGAVI [227R1A0572]

B.BHARATH RAJ [227R1A0573]

B.SAICHARAN [227R1A0568]

Under the guidance of

**Ms.G.LAVANYA**

Assistant Professor



**DEPARTMENT OF COMPUTER SCIENCE AND ENGINEERING**

# CMR TECHNICAL CAMPUS

**UGC AUTONOMOUS**

**Accredited by NBA & NAAC with ‘A’ Grade**

**Approved by AICTE, New Delhi and JNTUH Hyderabad Kandlakoya (V), Medchal Road, Hyderabad - 501401**

**December, 2023**

## **DEPARTMENT OF COMPUTER SCIENCE AND ENGINEERING**



## **CERTIFICATE**

This is to certify that the Real-Time (or) Field-based Research Project Report entitled **“ULTRASONIC SPECTACLES AND WAIST BELT FOR VISUALLY IMPAIRED AND BLIND PERSON”** being submitted by **B.BHARGAVI (227R1A0572) B.BHARATH RAJ (227R1A0573) B.SAICHARAN (227R1A0568)** in partial fulfillment of the requirements for the award of the degree of Bachelor of Technology in **COMPUTER SCIENCE AND ENGINEERING** to the **Jawaharlal Nehru Technological University, Hyderabad** is a record of bonafide work carried out by them under my guidance and supervision during the Academic Year 2023 – 24.

The results embodied in this thesis have not been submitted to any other University or Institute for the award of any other degree or diploma.

|  |  |
| --- | --- |
| **< Signature of the Supervisor>** | **< Signature of the HOD>** |
| **Ms.G.Lavanya** | **Dr. K. Srujan Raju** |
| **Assistant Professor** | **Head of the Department** |

**< Signature of the Director>**

**Dr. A. Raji Reddy**

**Director**

**ABSTRACT**

In this project presents an electronic navigation system for visually impaired and blind people (subject). This system understands obstacles around the subject up to 500 cm in front, left and right direction using a network of ultrasonic sensors. It effectively calculates distance of the detected object from the subject and prepares navigation path accordingly avoiding obstacles. It uses speech feedback to aware the subject about the detected obstacle and its distance. This proposed system uses AT89S52 microcontroller based embedded system to process real time data collected using ultrasonic sensor network. Based on direction and distance of detected obstacle, relevant pre-recorded speech message stored in APR9600 flash memory is invoked. Such speech messages are conveyed to the subject using earphone.

**TABLE OF CONTENTS**

**ABSTRACT i**

**1.INTRODUCTION 1**

1.1 PROJECT SCOPE 2

1.2 PROJECT PURPOSE 2

1.3 PROJECT FEATURES 3

1.3.1 ULTRASONIC SPECTACLES 3

1.3.2 ULTRSONIC WAIST BELT 3

1.3.3 BLUETOOTH INTEGRATION 3

1.3.4 SAFITY AND RELIABILITY 3

1.4 OBJECTIVES 4

**2.LITERATURE SURVEY** 6

2.1 ULTRASONIC SENSOR TECHNOLOGY 6

2.2 BLUETOOTH CONECTIVITY IN ASSISTIVE DEVICES 6

2.3 USER EXPERIENCE AND ACCEPTANCE 6

2.4 CHALLENGES AND FUTURE DIRECTIONS 7

**3.ANALYSIS AND DESIGN** 8

3.1 ANALYSIS 8

3.1.1 USER REQUIREMENTS 8

3.1.2 TECHNICAL REQUIREMENTS 8

3.1.3 SYSTEM COMPONENTS 8

3.2 DESIGN 9

3.2.1 ULTRASONIC SPECTACLES DESIGN 9

3.2.2 ULTRASONIC WAIST BELT DESIGN 9

3.2.3 BLUETOOTH INTRATION 9

3.2.4 SOFTWARE DESIGN 10

3.2.5 PROTOTYPING AND TESTING 10

3.3 PROBLEM DEFINITION 11

3.4 EXISTING SYSTEM 11

3.4.1 LIMITATIONS OF EXISTING SYSTEM 11

3.5 PROPOSED SYSTEM 11

3.6 HARDWARE COMPONENTS 12

3.6.1 ULTRASONIC SPECTACLES 12

3.6.2 ULTRASONIC WAIST BELT 12

3.7 SOFTWARE REQUIREMENTS 13

3.7.1 COMPANION MOBILE APPLICATION 13

3.7.2 FLASH PROGRAMMER 13

3.8 ARCHITECTURE 14

3.9 FEATURES 16

3.9.1 OBSTACLES DETECTION 16

3.9.2 REAL-TIME FEEDBACK 16

3.9.3 BLUETOOTH CONNECTIVITY 16

3.9.4 USER-FRIENDLY DESIGN 16

3.9.5 POWER EFFICIENCY 17

3.9.6 SAFETY AND RELIABILITY 17

3.9.7 CUSTOMIZABILITY 17

3.9.8 COMPANION APP FEATURES 18

**4.IMPLEMENTATION** 19

4.1 HARDWARE IMPLEMENTATION 19

4.1.1 ULTRASONIC SPECTACLES 19

4.1.2 ULTRASONIC WAIST BELT 19

4.1.3 POWER MANAGEMENT 19

4.2 SOFTWARE IMPLEMENTATION 20

4.2.1 EMBEDDED SOFTWARE 20

4.2.2 MOBILE APPLICATION 20

4.2.3 INTEGRATION AND TESTING 20

4.2.4 DEPLOYEMENT AND MAINTANANCE 20

4.2.5 TESTING AND CALIBRATION 21

4.3 SAMPLE CODE 22

**5.TESTING AND DEBUGGING/RESULTS** 25

5.1 FUNCTIONAL TESTING 25

5.2 PERFORMANCE TESTING 25

5.3USABILITY TESTING 26

5.4 ERROR HANDLIND AND DEBUGGING 26

5.5 RESULTS 27

**6.CONCLUSION**  29

**7.REFERENCES** 30

7.1 LINKS 30

**1.INTRODUCTION**

Navigating daily environments presents significant challenges for visually impaired and blind individuals, often compromising their safety and independence. Traditional mobility aids, such as white canes and guide dogs, offer valuable assistance but have inherent limitations in range and scope of obstacle detection. To address these gaps, the integration of advanced technologies into assistive devices has emerged as a promising solution.This project introduces an innovative assistive technology system designed to enhance the mobility, safety, and independence of visually impaired and blind individuals. The system comprises two main components: ultrasonic sensor-equipped spectacles and a waist-belt, both integrated with Bluetooth connectivity for enhanced functionality.The ultrasonic spectacles are designed to detect obstacles at head level, such as tree branches and signboards, which are often missed by traditional canes. Equipped with forward-facing ultrasonic sensors, the spectacles provide real-time auditory feedback through earphones, alerting the user to potential hazards and enabling them to navigate safely.Complementing the spectacles, the waist-belt features multiple ultrasonic sensors arranged to cover a 360-degree detection range around the user. This setup allows the belt to identify obstacles at ground and waist level, such as stairs, curbs, and low-hanging objects. Tactile feedback is provided through vibration motors, with varying intensity and patterns indicating the direction and proximity of obstacles.

The Bluetooth integration further enhances the system's capabilities, enabling seamless wireless connectivity with smartphones and other devices. Through a companion mobile app, users can customize feedback settings, monitor battery levels, and receive system updates. The app also facilitates easy calibration and adjustment of sensor sensitivity, ensuring the system meets individual needs and preferences.By combining ultrasonic technology with Bluetooth connectivity, this project aims to deliver a comprehensive and user-friendly solution that significantly improves the spatial awareness and mobility of visually impaired and blind individuals. The following sections will detail the design, functionality, and testing of the ultrasonic spectacles and waist-belt system, demonstrating its potential to enhance the quality of life for users by providing greater independence and confidence in navigating their surroundings. This introduction outlines the need for advanced assistive technologies for the visually impaired, the principles of ultrasonic obstacle detection, and the proposed solution of ultrasonic spectacles and a waist-belt. The following sections will delve into the design, functionality, and testing of the system, demonstrating its potential to significantly enhance the independence and quality of life for visually impaired and blind individuals.

**1.1 PROJECT SCOPE**

The project aims to develop a comprehensive assistive technology system incorporating ultrasonic sensors and Bluetooth connectivity to enhance the mobility, safety, and independence of visually impaired and blind individuals. The system includes ultrasonic sensor-equipped spectacles and a waist-belt designed to provide real-time feedback on the user's environment. The spectacles will have forward-facing ultrasonic sensors to detect head-level obstacles and provide auditory feedback through earphones.The project focuses on developing an advanced assistive technology system for visually impaired and blind individuals, combining ultrasonic spectacles and a waist-belt. The primary goals are to enhance the mobility, safety, and independence of users by providing real-time feedback on their surroundings.

**1.2 PROJECT PURPOSE**

The primary purpose of this project is to develop an advanced assistive technology system that significantly enhances the mobility, safety, and independence of visually impaired and blind individuals. By integrating ultrasonic sensors and Bluetooth connectivity into a pair of spectacles and a waist-belt, the system aims to provide real-time, multi-modal feedback to help users navigate their environments more effectively and confidently.The ultrasonic spectacles are designed to detect head-level obstacles, such as tree branches and signboards, which traditional mobility aids might miss. The system provides auditory alerts through earphones, informing the user of potential hazards and preventing collisions. The waist-belt, equipped with multiple ultra

sonic sensors, covers a 360-degree detection range to identify ground-level and waist-level obstacles, such as stairs, curbs, and low-hanging objects. It provides tactile feedback via vibration motors, with varying intensity and patterns indicating the direction and proximity of obstacles.Bluetooth connectivity enhances the system's functionality by allowing seamless integration with a companion mobile app. This app enables users to customize feedback settings, monitor battery levels, receive system updates, and adjust sensor sensitivity to suit individual needs and preferences. By offering both auditory and tactile feedback, the system ensures comprehensive spatial awareness, catering to different user preferences and environmental conditions.Ultimately, this project aims to deliver a practical, affordable, and user-friendly solution that empowers visually impaired and blind individuals to navigate their surroundings with greater independence, confidence, and safety.

**1.3 PROJECT FEATURES**

The ultrasonic sensor-equipped spectacles and waist belt system for visually impaired and blind individuals incorporate several advanced features to enhance mobility, safety, and independence, bolstered by Bluetooth connectivity for expanded functionality:

#### **1.3.1 Ultrasonic Spectacles**

* **Forward-Facing Ultrasonic Sensors**:
  + Detects head-level obstacles such as tree branches and signboards.
  + Provides real-time auditory alerts through integrated earphones.
* **Customizable Auditory Feedback**:
  + Offers adjustable volume and tone settings for personalized alerts.
  + Alerts users to the proximity and type of obstacles detected.
* **Comfort and Design**:
  + Lightweight, ergonomic design for all-day wearability.
  + Durable construction suitable for various environments.

**1.3.2 Ultrasonic Waist Belt**

* **Obstacle Detection**:
  + Multiple ultrasonic sensors cover a complete circumference around the user.
  + Detects ground-level obstacles like stairs, curbs, and low-hanging objects.
* **Tactile Feedback System**:
  + Utilizes vibration motors to provide tactile alerts.
  + Different vibration patterns and intensities indicate obstacle distance and direction.
* **Adjustable and Comfortable**:
  + Easily adjustable for different body sizes and preferences.
  + Designed with breathable materials for comfort during extended wear.

#### **1.3.3 Bluetooth Integration**

* **Wireless Connectivity**:
  + Enables seamless pairing with smartphones and other Bluetooth-enabled devices.
  + Facilitates data transmission between the assistive devices and a companion mobile app.
* **Companion Mobile App**:
  + User-friendly interface for customizing settings and preferences.
  + Monitors battery levels and provides alerts for recharging.

**1.3.4 Safety and Reliability**

* Advanced Signal Processing
* Long Battery Life
* Weatherproof and Durable

**1.4 OBJECTIVES**

* **Enhanced Obstacle Detection and Avoidance:**

Develop ultrasonic spectacles and waist belts capable of accurately detecting obstacles in the user's path using ultrasonic sensors. Ensure the system provides reliable distance measurements and immediate feedback through auditory signals or haptic vibrations, helping users navigate safely in both indoor and outdoor environments.

* **Bluetooth Integration for Connectivity:**

Integrate Bluetooth technology to enable seamless communication between the assistive device and external devices such as smartphones or tablets. This integration facilitates features like real-time data transmission, remote monitoring by caregivers or authorities, and configuration adjustments via a dedicated mobile application.

* **User-Centric Design and Interface:**

Design an intuitive user interface that caters to the needs of visually impaired individuals. Implement accessible controls, clear feedback mechanisms, and customizable settings (e.g., volume control, sensitivity adjustment) to accommodate varying user preferences and environmental conditions.

* **Long Battery Life and Efficient Power Management:**

Optimize power consumption to extend battery life, ensuring uninterrupted use over extended periods. Incorporate rechargeable batteries with a robust Battery Management System (BMS) to monitor and manage power efficiently, enhancing device reliability and reducing maintenance requirements.

* **Ergonomic and Durable Construction:**

Engineer the spectacles and waist belt with a focus on ergonomic comfort and durability. Utilize lightweight materials and ergonomic designs to enhance user comfort during prolonged wear. Ensure the devices are resilient to daily use and capable of withstanding environmental factors such as moisture and temperature fluctuations.

* **Reliability and Accuracy in Operation:**

Conduct thorough testing and calibration to validate the accuracy of obstacle detection and the reliability of Bluetooth connectivity. Ensure the system operates effectively across various lighting conditions, terrains, and obstacle types commonly encountered by visually impaired individuals.

* **Accessibility and Inclusivity:**

Ensure the design considers accessibility standards and the diverse needs of visually impaired users. Provide options for customization based on individual preferences and abilities, aiming to enhance usability and inclusivity for all users.

* **Safety Features and User Confidence:**

Prioritize user safety by promptly alerting them to potential obstacles and hazards in their surroundings. Equip the devices with safety features such as emergency alerts and automatic shut-off mechanisms to mitigate risks and enhance user confidence in independent navigation.

* **Community Engagement and Continuous Improvement:**

Engage with the visually impaired community and stakeholders throughout the development lifecycle. Solicit feedback through user trials, surveys, and focus groups to iteratively improve device features, functionality, and user experience based on real-world insights and needs.

* **Scalability and Affordability:**

Plan for scalability in manufacturing and distribution to ensure widespread availability of the assistive devices at affordable costs. Explore partnerships with organizations, governments, and funding opportunities to support accessibility initiatives and reduce financial barriers for end-users.

By systematically addressing these detailed objectives, ultrasonic spectacles and waist belts with Bluetooth integration can effectively empower visually impaired and blind individuals, offering enhanced mobility, safety, and independence in navigating their daily environments. This holistic approach aims to create impactful solutions that improve quality of life and promote greater inclusivity for all users.

**2.LITERATURE SURVEY**

A literature survey on the integration of ultrasonic sensors and Bluetooth technology in assistive devices for visually impaired and blind individuals reveals several studies and advancements focused on enhancing mobility, safety, and independence. Here are some key findings from existing literature:

**2.1. Ultrasonic Sensor Technology in Assistive Devices**

* **Obstacle Detection:** Ultrasonic sensors are widely used in assistive devices due to their ability to detect obstacles by emitting high-frequency sound waves and measuring the echo time. These sensors can accurately determine the distance and location of obstacles, providing crucial information for navigation (Babu et al., 2017).
* **Feedback Mechanisms:** The feedback systems in these devices commonly use auditory or tactile alerts to inform users of obstacles. Auditory feedback is delivered through earphones or speakers, while tactile feedback is provided via vibration motors. Customizable feedback settings are essential to cater to the diverse needs of users, ensuring the alerts are noticeable and not overwhelming (Chakraborty et al., 2019).

**2.2 Bluetooth Connectivity in Assistive Devices**

* **Wireless Communication:** Bluetooth technology enables wireless communication between the assistive device and a smartphone or companion app. This connectivity allows for real-time data transmission, remote monitoring, and easy adjustments of device settings. Users can customize their feedback preferences, monitor battery levels, and receive firmware updates through the app (Adler et al., 2018).
* **Companion Mobile Apps:** The development of user-friendly mobile applications is crucial. These apps provide a platform for users to interact with their assistive devices, offering features such as sensitivity adjustment, feedback customization, and real-time monitoring of device performance. The apps also facilitate training and support, enhancing user experience and adoption (Sahu et al., 2020).

**2.3 User Experience and Acceptance**

* **Design Considerations:** User-centric design is emphasized in the literature, focusing on comfort, usability, and aesthetics. The devices must be lightweight, ergonomic, and durable to ensure they can be worn comfortably throughout the day. Aesthetically pleasing designs also contribute to user acceptance (Goyal et al., 2021).
* **Field Testing and Feedback:** Extensive field testing is conducted to evaluate the effectiveness and practicality of these devices in real-world scenarios. Feedback from visually impaired users is critical in identifying issues and areas for improvement. Studies highlight the importance of involving users in the development process to create solutions that truly meet their needs (Kumar et al., 2022).

**2.4 Challenges and Future Directions**

* **Sensor Accuracy and Reliability:** Ensuring the accuracy and reliability of ultrasonic sensors in various environmental conditions remains a challenge. Research continues to focus on improving sensor technology and developing robust algorithms to minimize false positives and negatives (Singh et al., 2023).
* **Battery Life and Power Management:** The longevity of battery life is a critical factor for the practicality of wearable assistive devices. Efficient power management systems are being developed to extend battery life and reduce the frequency of recharging (Sharma et al., 2023).
* **Cost and Accessibility:** Making these advanced assistive technologies affordable and accessible to a broader population is a significant concern. Research is ongoing to find cost-effective solutions without compromising functionality and reliability.
* **Integration of AI and Machine Learning:** There is a growing interest in integrating artificial intelligence (AI) and machine learning into these devices. AI can enhance obstacle detection, adapt to user behavior, and provide predictive analytics to improve navigation and safety (Sharma et al., 2023).

The literature survey indicates that the integration of ultrasonic sensors and Bluetooth technology in assistive devices for visually impaired and blind individuals holds great promise. Significant progress has been made in developing reliable obstacle detection systems and user-friendly feedback mechanisms. However, challenges such as sensor accuracy, battery life, cost, and accessibility remain. Future research will likely focus on addressing these challenges and leveraging AI to further enhance the capabilities of these assistive devices.

**3.ANALYSIS AND DESIGN**

**3.1Analysis**

**3.1.1 User Requirements:**

* **Mobility Enhancement:** Enable visually impaired users to navigate safely and independently.
* **Obstacle Detection:** Accurately detect obstacles at head, waist, and ground levels.
* **Feedback Mechanisms:** Provide clear and intuitive feedback to users through auditory and tactile alerts.
* **Ease of Use:** Ensure the system is easy to operate, with minimal learning curve.
* **Comfort:** Ensure the device is comfortable to wear for extended periods.

**3.1.2 Technical Requirements:**

* **Sensor Accuracy:** Ultrasonic sensors must reliably detect obstacles within a specific range and angle.
* **Real-Time Processing:** Provide immediate feedback to users upon detecting obstacles.
* **Bluetooth Connectivity:** Enable wireless communication with a smartphone app for customization and monitoring.
* **Power Management:** Optimize battery life for prolonged use without frequent recharging.
* **Durability:** Devices must be weather-resistant and durable for daily use.

**3.1.3 System Components:**

* **Ultrasonic Sensors:** For obstacle detection.
* **Microcontroller:** To process sensor data and control feedback mechanisms.
* **Bluetooth Module:** For wireless communication.
* **Battery:** For powering the system.
* **Feedback Mechanisms:** Earphones for auditory feedback and vibration motors for tactile feedback.
* **Mobile Application:** For user customization and monitoring.

**3.2 Design**

**3.2.1 Ultrasonic Spectacles Design:**

* **Frame Design:**
  + Lightweight and ergonomic to ensure comfort.
  + Durable materials suitable for daily wear.
* **Sensor Placement:**
  + Ultrasonic sensors positioned on the front and sides of the spectacles.
  + Sensors should cover a horizontal field of view to detect obstacles at head level.
* **Microcontroller Integration:**
  + Embedded within the frame to process data from the sensors.
  + Ensure the microcontroller is small and lightweight.
* **Auditory Feedback:**
  + Earphones integrated into the spectacles.
  + Provide clear and distinguishable sounds indicating the proximity and direction of obstacles.
* **Power Supply:**
  + Rechargeable battery with efficient power management.
  + Battery compartment integrated into the frame.

**3.2.2 Ultrasonic Waist Belt Design:**

* **Belt Design:**
  + Adjustable and comfortable, made from breathable materials.
  + Durable construction to withstand daily use.
* **Sensor Placement:**
  + Multiple ultrasonic sensors placed around the belt to provide 360-degree coverage.
  + Sensors should detect obstacles at waist and ground levels.
* **Microcontroller Integration:**
  + Centrally located in the belt to process sensor data and control feedback mechanisms.
* **Tactile Feedback:**
  + Vibration motors placed around the belt.
  + Different vibration patterns and intensities to indicate the proximity and direction of obstacles.
* **Power Supply:**
  + Rechargeable battery with efficient power management.
  + Battery compartment integrated into the belt design.

**3.2.3 Bluetooth Integration:**

* **Bluetooth Module:**
  + Integrated into both the spectacles and the waist belt.
  + Ensure stable and efficient communication with the mobile app.
* **Mobile Application:**
  + User-friendly interface for customization and monitoring.
  + Features include:
    - Sensitivity adjustment for ultrasonic sensors.
    - Customization of auditory and tactile feedback.
    - Battery level monitoring.
    - Firmware updates and troubleshooting support.

**3.2.4 Software Design:**

* **Signal Processing Algorithms:**
  + Algorithms to process data from ultrasonic sensors.
  + Determine obstacle distance and direction accurately.
* **Feedback Control:**
  + Control the auditory and tactile feedback mechanisms based on processed data.
  + Ensure real-time response to detected obstacles.
* **Mobile App Development:**
  + Develop the app using a cross-platform framework to ensure compatibility with both Android and iOS.
  + Include features for real-time monitoring and user customization.

**3.2.5 Prototyping and Testing:**

* **Prototype Development:**
  + Create initial prototypes of the spectacles and waist belt.
  + Integrate all components and test for functionality.
* **User Testing:**
  + Conduct field tests with visually impaired users.
  + Gather feedback on usability, comfort, and effectiveness.
  + Iterate on the design based on user feedback.
* **Performance Testing:**
  + Test the system in various environments to ensure reliability and accuracy.
  + Evaluate battery life and power management.

The design and development of the ultrasonic sensor-equipped spectacles and waist belt with Bluetooth connectivity aim to provide a comprehensive assistive technology solution for visually impaired and blind individuals. By addressing the user and technical requirements, the system will offer enhanced mobility, safety, and independence. Continuous testing and iteration based on user feedback will ensure the final product is both effective and user-friendly.

**3.3 PROBLEM DEFINITION**

The primary problem faced by visually impaired and blind individuals is the difficulty in detecting and avoiding obstacles at various levels (head, waist, and ground) in real-time, which can lead to injuries and restrict their independence. Traditional mobility aids do not provide adequate detection of all obstacles, especially those that are head-level or unexpected, like low-hanging branches or protruding objects. Moreover, these aids do not offer feedback that is customizable to the user's needs and preferences.

**3.4 EXISTING SYSTEM**

Ultrasonic canes, also known as electronic travel aids (ETAs), are traditional mobility aids enhanced with ultrasonic sensors. These devices emit ultrasonic waves to detect obstacles and provide auditory or tactile feedback to the user. Smart glasses for visually impaired individuals integrate cameras and sensors, including ultrasonic sensors, to detect obstacles and provide feedback through auditory signals. Waist belts equipped with ultrasonic sensors are designed to detect obstacles around the user and provide tactile feedback through vibration motors embedded in the belt. These systems combine both glasses and waist belts equipped with ultrasonic sensors to provide comprehensive obstacle detection at different levels and directions.

**3.4.1 LIMITATIONS OF EXISTING SYSTEM:**

* **Limited Detection Range:** Can only detect obstacles in the immediate path and at ground level.
* **Comfort:** Some designs may be bulky or uncomfortable to wear for extended periods. **Bluetooth Connectivity:** Some models include Bluetooth connectivity to a companion app for customization and monitoring.
* **Battery Life:** High power consumption leading to shorter battery life.
* **Complexity:** May be complex to use and require significant user adaptation.
* **Cost:** Generally expensive due to advanced technologies.

**3.5 PROPOSED SYSTEM**

* Automatic voice indication based on different places.
* Wireless transmission.
* Automatic data collection system.

**3.6 HARDWARE REQUIREMENT**

**3.6.1 Ultrasonic Spectacles:**

* **Ultrasonic Sensors:** High-precision sensors to detect obstacles at head level.
* **Microcontroller:** A compact and efficient microcontroller (e.g., Arduino Nano, ESP32) to process sensor data.
* **Earphones:** Integrated or detachable earphones for auditory feedback.
* **Bluetooth Module:** For wireless connectivity with the mobile app (e.g., HC-05, BLE).
* **Rechargeable Battery:** Lightweight battery with sufficient capacity for extended use (e.g., Li-ion or Li-Po battery).
* **Frame Material:** Durable and lightweight materials like plastic or titanium for the frame.
* **Wiring and Connectors:** For connecting sensors, microcontroller, and feedback devices.
* **Enclosure:** Protective casing for electronic components.

**3.6.2 Ultrasonic Waist Belt:**

* **Ultrasonic Sensors:** Multiple sensors to provide 360-degree obstacle detection.
* **Microcontroller:** To process data from multiple sensors and control feedback mechanisms.
* **Vibration Motors:** Embedded around the belt for tactile feedback.
* **Bluetooth Module:** For connectivity with the mobile app.
* **Rechargeable Battery:** High-capacity battery to ensure long usage times.
* **Belt Material:** Adjustable, breathable, and durable materials for comfort.
* **Wiring and Connectors:** For sensor and motor integration.
* **Enclosure:** Protective casing for electronic components.

**3.7 SOFTWARE REQUIREMENTS:**

**3.7.1 Companion Mobile Application:**

* **Development Environment:**
  + **Android:** Android Studio, Java/Kotlin.
  + **iOS:** Xcode, Swift.
  + **Cross-Platform Options:** React Native, Flutter, Xamarin.
* **Core Functionalities:**
  + **Sensor Calibration and Sensitivity Settings:** User interface to adjust sensor settings.
  + **Feedback Customization:** Options to customize auditory and tactile feedback.
  + **Real-Time Monitoring:** Display of sensor data and system status.
  + **Battery Level Indicator:** Monitor the battery status of the spectacles and waist belt.
  + **Firmware Updates:** Over-the-air (OTA) updates for the devices.


**3.7.2 Flash Programmer**

* A flash programmer is essential for loading compiled firmware/software (often in binary form) into the flash memory of microcontrollers, microprocessors, or other programmable devices.
* It allows for the initial programming of a device or updating/reprogramming of firmware during development, manufacturing, or in-field updates.
* Used in embedded systems development, production programming, and field updates of devices.
* Essential in industries such as automotive, consumer electronics, industrial automation, and telecommunications.

The proposed system's hardware and software requirements are designed to ensure comprehensive obstacle detection, intuitive feedback, and user-friendly customization for visually impaired and blind individuals. By integrating advanced components and robust software, the system aims to provide enhanced mobility, safety, and independence.

Top of Form

**3.8 ARCHITECTURE**

****

Bottom of Form

**MICRO CONTROLLER:**

A microcontroller is a compact integrated circuit designed to govern a specific operation in an embedded system. For the ultrasonic sensor and waist belt system for visually impaired and blind individuals with Bluetooth connectivity, the microcontroller serves as the brain of the device, managing sensor data processing, feedback mechanisms, and Bluetooth communication. The microcontroller processes this sensor data in real time and generates appropriate feedback, such as auditory signals or vibrations, to alert the user about nearby obstacles. Key considerations for selecting a microcontroller include sufficient processing power to handle real-time data, low power consumption to maximize battery life, support for necessary peripherals like ADC for sensor data and PWM for haptic feedback, compact size to fit within wearable devices, and robust development support for efficient development and debugging.in this we use (P89V51/AT89s51) microcontroller.

**MICROCONTROLLER (P89V51/AT89s51):**

The P89V51 and AT89S51 microcontrollers, both part of the 8051 family, are well-suited for embedded applications such as ultrasonic spectacles and waist belts for visually impaired and blind individuals. These microcontrollers are integral in processing data from ultrasonic sensors, managing power consumption, and generating feedback signals to alert users about obstacles. Both microcontrollers are designed for low power consumption, essential for wearable devices. In ultrasonic spectacles and waist belts, these microcontrollers collect and process sensor data to detect obstacles, generate auditory or haptic feedback, manage power efficiently, and handle user interface controls. Their robust architecture and versatility make them reliable and practical choices for enhancing the mobility and safety of visually impaired individuals, offering greater independence and confidence in navigating their environments.

**ULTRASONIC SENSOR:**

Ultrasonic sensors are a pivotal component in the waist belt and spectacles system for visually impaired and blind individuals. These sensors use ultrasonic waves to detect obstacles and provide critical data to the microcontroller, which then processes this information to assist users in navigating their environment safely. These sensors provide real-time obstacle detection and immediate feedback, enhancing situational awareness and mobility for users. Their discreet design and ease of integration with microcontrollers make them practical for wearable devices, thereby improving the safety and independence of visually impaired individuals.

**POWER SUPPLY:**

The power supply must provide the appropriate voltage levels required by the various components of the system. Common operating voltages for microcontrollers and sensors are 3.3V and 5V. The power supply for ultrasonic spectacles and waist belts is a critical component, ensuring these assistive devices operate reliably and continuously. Given the portability and lightweight requirements of wearable technology, rechargeable batteries such as Lithium-Ion (Li-Ion) or Lithium-Polymer (Li-Po) are ideal due to their high energy density, stable output, and compact form factor.

**VOICE ANNUNCIATOR:**

A voice annunciator is a crucial component integrated into ultrasonic spectacles and waist belts designed for visually impaired and blind individuals. This device enhances safety and navigation by providing auditory alerts and announcements based on real-time sensor data. The voice annunciator utilizes synthesized speech to convey information about obstacles, distances, and other relevant environmental cues to the user.

**3.10 FEATURES**

**3.8.1 Obstacle Detection**

* **Ultrasonic Sensors:**
  + **Head-Level Detection:** Sensors placed on spectacles to detect obstacles at head height.
  + **Waist-Level Detection:** Sensors on the waist belt to identify obstacles at waist level.
  + **Ground-Level Detection:** Sensors to detect obstacles and changes in elevation on the ground.

#### **3.8.2. Real-Time Feedback**

* **Auditory Feedback:**
  + **Headphones or Bone Conduction Speakers:** Provide sound alerts about the direction and distance of obstacles.
  + **Customizable Alerts:** Different tones or spoken warnings to indicate varying levels of proximity to obstacles.
* **Tactile Feedback:**
  + **Vibration Motors:** Integrated into the waist belt to provide haptic feedback.
  + **Directional Vibrations:** Different vibration patterns indicating the direction (front, sides, back) and urgency of the obstacle.

#### **3.8.3 Bluetooth Connectivity**

* **Wireless Communication:**
  + **Mobile App Integration:** Connects to a companion app on a smartphone via Bluetooth.
  + **Settings Configuration:** Allows users to customize feedback settings, sensitivity, and alerts through the app.
  + **Firmware Updates:** Wireless updates to improve system functionality and add new features.

#### **3.8.4 User-Friendly Design**

* **Ergonomic Design:**
  + **Comfortable Wearability:** Lightweight and ergonomically designed spectacles and waist belt for extended use.
  + **Adjustable Fit:** Adjustable straps and components to fit different body types and sizes comfortably.
* **Ease of Use:**
  + **Simple Controls:** Easy-to-use buttons or touch interface on the waist belt for quick adjustments and power management.
  + **Voice Commands:** Potential for integration with voice assistants for hands-free operation.

#### **3.8.5 Power Efficiency**

* **Battery Life:**
  + **Long-Lasting Battery:** Efficient power management to extend battery life, allowing for prolonged use between charges.
  + **Rechargeable Battery:** Integrated rechargeable battery with USB charging capability for convenience.
* **Power Management:**
  + **Sleep Mode:** Automatically enters low power mode when not in use to conserve battery.
  + **Battery Status Indicators:** LED indicators or app-based notifications to inform the user of battery status and charging needs.

#### **3.8.6 Safety and Reliability**

* **Robust Construction:**
  + **Durability:** Built to withstand daily wear and tear, with resistance to dust and moisture for reliable outdoor use.
  + **Safety Features:** Overvoltage and short-circuit protection in the power supply for user safety.
* **Accurate Sensing:**
  + **High Precision:** Accurate distance measurement and quick response time to ensure reliable obstacle detection.
  + **Wide Detection Range:** Sufficient range to detect obstacles in a typical walking environment, ensuring comprehensive coverage.

#### **3.8.7 Customizability**

* **Adjustable Sensitivity:**
  + **User Preferences:** Users can adjust the sensitivity of the ultrasonic sensors to suit different environments and personal preferences.
  + **Environment Modes:** Preset modes for different environments (e.g., indoor, outdoor, crowded areas) to optimize performance.
* **Feedback Customization:**
  + **Alert Preferences:** Users can choose between different types of alerts (sound, vibration, or both) based on their preferences and needs.
  + **Volume and Intensity:** Adjustable volume for auditory feedback and intensity for vibrations.

**3.8.8 Companion App Features**

* **Real-Time Monitoring:**
  + **Obstacle Tracking:** Visual representation of detected obstacles on the app for additional situational awareness.
  + **Navigation Assistance:** Integration with GPS for route guidance and safe path suggestions.
* **User Analytics:**
  + **Usage Statistics:** Tracks usage patterns and obstacle encounters to help users understand and improve their mobility.
  + **Health Monitoring:** Potential integration with health tracking features (e.g., step count, activity levels).

By combining these features, the ultrasonic sensor and waist belt system with Bluetooth connectivity offer a comprehensive assistive technology solution, significantly enhancing the mobility, safety, and independence of visually impaired and blind individuals.

**4.IMPLEMENTATION**

Implementing an ultrasonic sensor and waist belt system for visually impaired and blind individuals with Bluetooth involves several steps and considerations to ensure functionality, usability, and effectiveness. Here’s an overview of the implementation process:

### Implementation of Ultrasonic Sensor and Waist Belt

#### **System Design:**

* **Requirement Gathering:** Understand the specific needs and challenges of visually impaired users regarding mobility and obstacle detection.
* **Component Selection:** Choose appropriate ultrasonic sensors, microcontrollers, vibration motors, Bluetooth modules, and power sources based on performance, power consumption, and compatibility.
* **Design Specifications:** Define the detection range, feedback mechanisms (auditory and tactile), and user interface (via a mobile app).

#### **4.1 Hardware Implementation:**

**4.1.1 Ultrasonic Spectacles:**

* Integrate ultrasonic sensors into the spectacles' frame to detect head-level obstacles.
* Connect sensors to a microcontroller (e.g., Arduino Nano or ESP32) for data processing.
* Incorporate earphones or bone conduction transducers for auditory feedback.
* Ensure Bluetooth connectivity for communication with the mobile app.

**4.1.2 Ultrasonic Waist Belt:**

* Position multiple ultrasonic sensors around the waist belt for 360-degree obstacle detection.
* Interface sensors with a microcontroller for sensor data processing.
* Embed vibration motors strategically along the belt for tactile feedback.
* Include a Bluetooth module for wireless connectivity with the mobile app.

**4.1.3 Power Management:**

* Select and integrate rechargeable batteries with adequate capacity and efficient power management to ensure extended operational time

#### 4.2 **Software Implementation:**

**4.2.1 Embedded Software (Microcontroller):**

* Develop firmware using Arduino IDE or similar platforms to control sensor data acquisition, feedback mechanisms, and Bluetooth communication.
* Implement algorithms for obstacle detection, distance calculation, and feedback generation (auditory tones and vibration patterns).
* Ensure robust error handling and reliability in data transmission.

**4.2.2 Mobile Application:**

* Develop a mobile app (for Android and/or iOS) with a user-friendly interface.
* Implement Bluetooth Low Energy (BLE) communication protocols for seamless connectivity with the spectacles and waist belt.
* Design the app to allow users to customize feedback settings (e.g., sensitivity adjustment, feedback type).
* Include features for real-time monitoring of device status (battery level, sensor performance).
* Provide firmware update capabilities to ensure the system remains up-to-date with the latest features and improvements.

#### **4.2.3 Integration and Testing:**

* **Hardware Integration:** Assemble all components into the spectacles and waist belt, ensuring proper fit, comfort, and functionality.
* **Software Integration:** Pair the devices with the mobile app and test Bluetooth connectivity and data exchange.
* **Functional Testing:** Conduct rigorous testing to verify obstacle detection accuracy, feedback responsiveness, and overall system performance.
* **User Testing:** Involve visually impaired individuals in usability testing to gather feedback and make necessary adjustments for intuitive operation.

#### **4.2.4** **Deployment and Maintenance:**

* **Deployment:** Deploy the system in controlled environments and gather real-world feedback from users.
* **Maintenance:** Provide ongoing support, including troubleshooting guides and software updates to enhance functionality and address user feedback.

Implementing an ultrasonic sensor and waist belt system for visually impaired and blind individuals with Bluetooth involves careful planning, selection of components, robust software development, and thorough testing.

#### **4.2.5 Testing and Calibration**

* **Functional Testing:**
  + Conduct comprehensive testing to validate the accuracy of obstacle detection, reliability of voice annunciator alerts, and overall system performance.
  + Test the device in various environments and conditions typical for visually impaired individuals to ensure robustness and effectiveness.
* **User Feedback and Iteration:**
  + Engage visually impaired users in beta testing to gather feedback on usability, clarity of alerts, and overall user experience.
  + Use feedback to refine software algorithms, adjust alert parameters, and improve the design for better integration into daily use.

#### **4.2.6 Deployment and Maintenance**

* **Manufacturing and Deployment:**
  + Scale up production based on finalized designs and testing results, ensuring consistency and quality in manufacturing processes.
  + Deploy the devices to users, providing necessary documentation, training, and support to ensure proper use and maintenance.
* **Continuous Improvement:**
  + Establish a framework for ongoing maintenance, including software updates, bug fixes, and enhancements based on user feedback and technological advancements.
  + Monitor device performance in the field and implement improvements to meet evolving user needs and regulatory requirements.

Implementing a voice annunciator in ultrasonic spectacles and waist belts involves a systematic approach encompassing hardware integration, software development, rigorous testing, and user engagement. By focusing on reliability, usability, and user feedback, these devices can effectively enhance the safety, mobility, and independence of visually impaired and blind individuals in navigating their surroundings. Continued innovation and refinement ensure that these assistive technologies meet the highest standards of functionality and accessibility.

**4.3 SAMPLE CODE:**

#include <LiquidCrystal.h>

#include <stdio.h>

#include <SoftwareSerial.h>

SoftwareSerial mySerial(A4, A5);

LiquidCrystal lcd(6, 7, 5, 4, 3, 2);

const int trigPin = 8;

const int echoPin = 9;

int buzzer = 13;

int rtr1=0;

int dist1=0,dist2=0,dist3,sts1=0,sts2=0;

long duration;

int distanceCm, distanceInch;

unsigned char rcv,count,gchr='x',gchr1='x',robos='s';

char pastnumber[10];

char gpsval[50];

// char dataread[100] = "";

// char lt[15],ln[15];

int i=0,k=0;

int gps\_status=0;

float latitude=0;

float logitude=0;

String Speed="";

String gpsString="";

char \*test="$GPRMC";

int hbtc=0,hbtc1=0,rtrl=0;

unsigned char gv=0,msg1[10],msg2[11];

float lati=0,longi=0;

unsigned int lati1=0,longi1=0;

unsigned char flat[5],flong[5];

unsigned char finallat[8],finallong[9];

int ii=0;

float tempc=0,weight=0;

float vout=0;

String inputString = ""; // a string to hold incoming data

boolean stringComplete = false; // whether the string is complete

unsigned int ultra\_dist()

{int ud=0;

digitalWrite(trigPin, LOW);

delayMicroseconds(2);

digitalWrite(trigPin, HIGH);

delayMicroseconds(10);

digitalWrite(trigPin, LOW);

duration = pulseIn(echoPin, HIGH);

}

void setup()

{

Serial.begin(9600);

mySerial.begin(9600);

pinMode(trigPin, OUTPUT); // Sets the trigPin as an Output

pinMode(echoPin, INPUT); // Sets the echoPin as an Input

pinMode(buzzer, OUTPUT);

digitalWrite(buzzer, HIGH);

lcd.begin(16, 2);lcd.cursor();

lcd.print("Ultrasonic Specticles");

lcd.setCursor(0,1);

lcd.print("Wastbelt Visually");

delay(2000);

lcd.clear();

lcd.setCursor(0,0);

lcd.print("U:");//3-4-5-6-7,0

}

int dista=0;

void loop()

{

dista=0;

dist1=0;

dist2=0;

for(rtr1=0;rtr1<5;rtr1++)

{

dista = ultra\_dist();

delay(10);

}

dist1 = (dist1/5);

lcd.setCursor(3,0);lcd.print(dist1);lcd.print(" ");delay(10);

if(dist1 < 10)

{

lcd.setCursor(0,1);lcd.print("Obstcale Detected");

Serial.println("Obstacle Detected");delay(1000);

Serial.println("Obstacle Detected");delay(1000);

lcd.setCursor(0,1);lcd.print(" ");

}

}

**5.TESTING AND DEBUGGING/RESULTS**

Testing and debugging an ultrasonic sensor and waist belt system designed for visually impaired and blind individuals, integrated with Bluetooth connectivity, is crucial to ensure functionality, reliability, and user satisfaction. Here’s a detailed approach to testing and debugging such a system:

### **5.1Functional Testing:**

* **Obstacle Detection:**
  + **Scenario Simulation:** Create diverse environments (indoor, outdoor) with obstacles at different heights and distances.
  + **Verification:** Ensure ultrasonic sensors accurately detect obstacles at head, waist, and ground levels.
  + **Distance Accuracy:** Validate sensor readings under varying environmental conditions (noise, lighting) to ensure reliable obstacle detection.
* **Feedback Mechanisms:**
  + **Auditory Feedback:** Test clarity and understandability of auditory alerts delivered through earphones or bone conduction transducers.
  + **Tactile Feedback:** Verify effectiveness of vibration patterns from the waist belt in indicating obstacle proximity and direction.
  + **Customization:** Test ability to adjust feedback settings (volume, vibration intensity) via the mobile app and verify changes take effect promptly.

#### **Bluetooth Connectivity:**

* **Pairing and Connection:**
  + **Mobile App Integration:** Ensure seamless pairing of spectacles and waist belt with the mobile app using Bluetooth Low Energy (BLE).
  + **Data Exchange:** Verify reliable transmission of sensor data (obstacle detection, feedback signals) between devices and app.
  + **Stability:** Test connectivity stability and latency to ensure real-time updates and commands are delivered without delays.

#### 5.2 **Performance Testing:**

* **Battery Life:** Assess power consumption and battery longevity during typical usage scenarios to ensure adequate endurance.
* **Durability:** Test robustness of hardware components (sensors, vibration motors) against wear and environmental conditions.
* **Reliability:** Conduct stress tests to evaluate system performance over extended periods and under varying loads.

#### 5.3 **Usability Testing:**

* **User Interaction:** Involve visually impaired individuals in usability tests to evaluate ease of setup, operation, and adjustment of settings.
* **Feedback Collection:** Gather user feedback on effectiveness of obstacle detection and clarity of feedback mechanisms.
* **Accessibility:** Ensure mobile app interface and controls are accessible and intuitive for users with visual impairments.

#### 5.4 **Error Handling and Debugging:**

* **Error Detection:** Implement robust error handling mechanisms to detect and recover from communication failures or sensor inaccuracies.
* **Log Analysis:** Analyze system logs and error reports to identify and address software bugs or performance issues promptly.
* **Iteration and Improvement:** Iterate on the system based on testing feedback to enhance functionality, user experience, and overall reliability.

Testing and debugging an ultrasonic sensor and waist belt system for visually impaired and blind individuals with Bluetooth involves rigorous verification of obstacle detection, feedback mechanisms, Bluetooth connectivity, performance under various conditions, and usability by the target users. By systematically testing each component and actively engaging users in the testing process, developers can refine the system to deliver a reliable and effective assistive technology solution that enhances mobility and independence for visually impaired individuals. Continuous iteration and improvement based on testing outcomes are crucial to optimizing the system’s performance and ensuring user satisfaction in real-world applications.

**5.5 RESULTS**



As of my last update, specific results detailing the performance and outcomes of ultrasonic sensor and waist belt systems designed for visually impaired and blind individuals with Bluetooth connectivity are not readily available. However, here are some anticipated or expected results based on typical objectives and goals of such systems:

### **Expected Results of Ultrasonic Sensor and Waist Belt System**

#### **Enhanced Obstacle Detection:**

* **Accurate Detection:** The system should accurately detect obstacles at head, waist, and ground levels, providing users with timely and reliable information.
* **360-Degree Coverage:** Waist belt sensors should offer comprehensive 360-degree coverage around the user, ensuring awareness of obstacles from all directions.

#### **Effective Feedback Mechanisms:**

* **Auditory Feedback:** Users should receive clear and understandable auditory alerts through earphones or bone conduction transducers, indicating obstacle distance and direction.
* **Tactile Feedback:** Vibration patterns from the waist belt should effectively convey obstacle proximity and direction through intuitive tactile sensations.

#### **Bluetooth Connectivity:**

* **Reliable Connection:** Bluetooth connectivity should be stable, enabling seamless communication between the spectacles, waist belt, and the companion mobile app.
* **Real-Time Updates:** Users should experience minimal latency in receiving real-time updates and adjustments to feedback settings via the mobile app.

#### **User Experience and Usability:**

* **Ease of Use:** The system should be user-friendly, allowing for straightforward setup, operation, and customization of feedback settings.
* **Comfort and Fit:** Spectacles and waist belt should be comfortable to wear for extended periods, designed with materials that promote breathability and durability.

#### **Battery Performance:**

* **Longevity:** The system’s battery life should be sufficient for daily use, with efficient power management strategies to maximize operational uptime.
* **Rechargeability:** Users should find it convenient to recharge the batteries, ensuring minimal downtime between charges.

#### **Safety and Independence:**

**Enhanced Mobility:** Users should experience increased confidence and independence in navigating their surroundings, aided by the system’s obstacle detection and feedback capabilities.

The ultimate success of an ultrasonic sensor and waist belt system for visually impaired and blind individuals with Bluetooth hinges on achieving these expected results. Real-world testing and user feedback are crucial for validating these outcomes and iterating on the system to continually improve functionality, reliability, and user satisfaction. As advancements in technology and user-centric design continue, these systems are poised to make significant contributions to enhancing the quality of life and independence for individuals with visual impairments.

**6.CONCLUSION**

In conclusionThe ultrasonic sensor and waist belt system integrated with Bluetooth technology represents a transformative solution for visually impaired and blind individuals, aimed at enhancing their mobility and safety. This innovative system utilizes ultrasonic sensors strategically placed in both spectacles and a waist belt to detect obstacles at head, waist, and ground levels, providing comprehensive 360-degree coverage. Through Bluetooth connectivity, the system communicates seamlessly with a companion mobile app, enabling users to customize feedback settings and receive real-time updates on obstacle proximity and direction. Auditory feedback delivered through earphones or bone conduction transducers offers clear alerts, while tactile feedback via vibration motors in the waist belt provides intuitive cues for navigation. Designed with user comfort and usability in mind, the system promotes independence by empowering users to confidently navigate diverse environments, minimizing the risk of collisions and enhancing overall safety. As technology continues to evolve, ongoing improvements in accuracy, integration, and user experience promise to further enhance the effectiveness and adoption of these assistive technologies, ultimately contributing to a more inclusive and accessible society.

**7. REFERENCES**

[1] Babu, S., et al. (2017). "Ultrasonic Aid for Visually Impaired People." International Journal of Advanced Research in Electronics and Communication Engineering, 6(5), 92-97.

[2] Adler, R., et al. (2018). "Bluetooth-Based Smart Device for the Blind and Visually Impaired." Journal of Assistive Technologies, 12(1), 23-31.

[3] Akshay Sharma A S, “ Review on Ultrasonic spectacles and waist belt”, International Research Journal of Engineering and Technology(IRJET),vol-09,issue no-07,pp.725-726,2020

[4] Chakraborty, S., et al. (2019). "Ultrasonic Blind Walking Stick Using Arduino and GSM." International Journal of Engineering Research and Applications, 9(1), 10-14.

[5] Sahu, A. K., et al. (2020). "Smart Assistive Belt for Visually Impaired People." Journal of Medical Systems, 44(6), 110.

[6] Goyal, R., et al. (2021). "Smart Cane for the Visually Impaired Using IoT." International Journal of Scientific Research in Computer Science, Engineering and Information Technology, 6(4), 7-11.

[7] Kumar, A., et al. (2022). "IoT-Based Navigation System for the Blind and Visually Impaired Using Ultrasonic Sensors and Raspberry Pi." International Journal of Computer Science and Information Security, 20(2), 112

**LINKS**

<https://www.researchgate.net/publication/261163651_Ultrasonic_spectacles_and_waist-belt_for_visually_impaired_and_blind_person>

[(72) IOSR Journal of Engineering (IOSRJEN) Ultrasonic Spectacles & Waist-Belt for Visually Impaired & Blind Person | IOSR Journal of Engineering - Academia.edu](https://www.academia.edu/6329699/IOSR_Journal_of_Engineering_IOSRJEN_Ultrasonic_Spectacles_and_Waist_Belt_for_Visually_Impaired_and_Blind_Person)